Manpage of INTRO

# INTRO

Section: Misc. Reference Manual Pages (3T)
Updated: August 21, 1997
Index
Return to Main Contents

## NAME

libtiff - introduction to libtiff, a library for reading and writing TIFF files

## SYNOPSIS

#include <tiffio.h>
cc file.c -ltiff

## DESCRIPTION

libtiff is a library for reading and writing data files encoded with the Tag Image File format, Revision 6.0 (or revision 5.0 or revision 4.0). This file format is suitable for archiving multi-color and monochromatic image data.

The library supports several compression algorithms, as indicated by the Compression field, including: no compression (1), CCITT 1D Huffman compression (2), CCITT Group 3 Facsimile compression (3), CCITT Group 4 Facsimile compression (4), Lempel-Ziv & Welch compression (5), baseline JPEG compression (7), word-aligned 1D Huffman compression (32771), and PackBits compression (32773). In addition, several nonstandard compression algorithms are supported: the 4-bit compression algorithm used by the ThunderScan program (32809) (decompression only), NeXT's 2-bit compression algorithm (32766) (decompression only), an experimental LZ-style algorithm known as Deflate (32946), and an experimental CIE LogLuv compression scheme designed for images with high dynamic range (32845 for LogL and 32845 for LogLuv). Directory information may be in either little- or big-endian byte order-byte swapping is automatically done by the library. Data bit ordering may be either Most Significant Bit (MSB) to Least Significant Bit (LSB) or LSB to MSB. Finally, the library does not support files in which the BitsPerSample, Compression, MinSampleValue, or MaxSampleValue fields are defined differently on a per-sample basis (in Rev. 6.0 the Compression tag is not defined on a per-sample basis, so this is immaterial).

## DATA TYPES

The library makes extensive use of C typedefs to promote portability. Two sets of typedefs are used, one for communication with clients of the library and one for internal data structures and parsing of the TIFF format. The following typedefs are exposed to users either through function definitions or through parameters passed through the varargs interfaces.

    typedef unsigned short uint16;        16-bit unsigned integer
    typedef unsigned <thing> uint32;      32-bit unsigned integer

    typedef unsigned int ttag_t;          directory tag
    typedef uint16 tdir_t;                directory index
    typedef uint16 tsample_t;             sample number
    typedef uint32 tstrip_t;              strip number
    typedef uint32 ttile_t;               tile number
    typedef int32 tsize_t;                i/o size in bytes
    typedef void* tdata_t;                image data ref
    typedef void* thandle_t;              client data handle
    typedef int32 toff_t;                 file offset

Note that tstrip_t, ttile_t, and tsize_t are constrained to be no more than 32-bit quantities by 32-bit fields they are stored in in the TIFF image. Likewise tsample_t is limited by the 16-bit field used to store the SamplesPerPixel tag. tdir_t constrains the maximum number of IFDs that may appear in an image and may be an arbitrary size (w/o penalty). ttag_t must be either int, unsigned int, pointer, or double because the library uses a varargs interface and ANSI C restricts the type of the parameter before an ellipsis to be a promoted type. toff_t is defined as int32 because TIFF file offsets are (unsigned) 32-bit quantities. A signed value is used because some interfaces return -1 on error. Finally, note that user-specified data references are passed as opaque handles and only cast at the lowest layers where their type is presumed.

## LIST OF ROUTINES

The following routines are part of the library. Consult specific manual pages for details on their operation. The manual page names listed below are for systems where the full function names can not be encoded in the filesystem; on most systems doing ``man function-name'' will work.

    Name                   Appears on Page  Description

    TIFFCheckTile          tile.3t          very x,y,z,sample is within image
    TIFFClientOpen         open.3t          open a file for reading or writing
    TIFFClose              close.3t         close an open file
    TIFFComputeStrip       strip.3t         return strip containing y,sample
    TIFFComputeTile        tile.3t          return tile containing x,y,z,sample
    TIFFCurrentDirectory   query.3t         return index of current directory
    TIFFCurrentRow         query.3t         return index of current scanline
    TIFFCurrentStrip       query.3t         return index of current strip
    TIFFCurrentTile        query.3t         return index of current tile
    TIFFError              error.3t         library error handler
    TIFFFdOpen             open.3t          open a file for reading or writing
    TIFFFileName           query.3t         return name of open file
    TIFFFileno             query.3t         return open file descriptor
    TIFFFlush              flush.3t         flush all pending writes
    TIFFFlushData          flush.3t         flush pending data writes
    TIFFGetBitRevTable     swab.3t          return bit reversal table
    TIFFGetField           getfield.3t      return tag value in current directory
    TIFFGetFieldDefaulted  getfield.3t      return tag value in current directory
    TIFFGetMode            query.3t         return open file mode
    TIFFGetVersion         query.3t         return library version string
    TIFFIsTiled            query.3t         return true if image data is tiled
    TIFFIsByteSwapped      query.3t         return true if image data is byte-swapped
    TIFFNumberOfStrips     strip.3t         return number of strips in an image
    TIFFNumberOfTiles      tile.3t          return number of tiles in an image
    TIFFOpen               open.3t          open a file for reading or writing
    TIFFPrintDirectory     print.3t         print description of the current directory
    TIFFReadBufferSetup    rdbuf.3t         specify i/o buffer for reading
    TIFFReadDirectory      readdir.3t       read the next directory
    TIFFReadEncodedStrip   rdestrip.3t      read and decode a strip of data
    TIFFReadEncodedTile    rdetile.3t       read and decode a tile of data
    TIFFReadRawStrip       rdrstrip.3t      read a raw strip of data
    TIFFReadRawTile        rdrtile.3t       read a raw tile of data
    TIFFReadRGBAImage      rdimage.3t       read an image into a fixed format raster
    TIFFReadScanline       readline.3t      read and decode a row of data
    TIFFReadTile           readtile.3t      read and decode a tile of data
    TIFFReverseBits        swab.3t          reverse bits in an array of bytes
    TIFFRGBAImageBegin     rgbaimage.3t     setup decoder state for TIFFRGBAImageGet
    TIFFRGBAImageEnd       rgbaimage.3t     release TIFFRGBAImage decoder state
    TIFFRGBAImageGet       rgbaimage.3t     read and decode an image
    TIFFRGBAImageOK        rgbaimage.3t     is image readable by TIFFRGBAImageGet
    TIFFScanlineSize       size.3t          return size of a scanline
    TIFFSetDirectory       setdir.3t        set the current directory
    TIFFSetSubDirectory    setdir.3t        set the current directory
    TIFFSetErrorHandler    error.3t         set error handler function
    TIFFSetField           setfield.3t      set a tag's value in the current directory
    TIFFSetWarningHandler  error.3t         set warning handler function
    TIFFStripSize          size.3t          return size of a strip
    TIFFSwabShort          swab.3t          swap bytes of short
    TIFFSwabLong           swab.3t          swap bytes of long
    TIFFSwabArrayOfShort   swab.3t          swap bytes of an array of shorts
    TIFFSwabArrayOfLong    swab.3t          swap bytes of an array of longs
    TIFFTileRowSize        size.3t          return size of a row in a tile
    TIFFTileSize           size.3t          return size of a tile
    TIFFVGetField          getfield.3t      return tag value in current directory
    TIFFVGetFieldDefaulted getfield.3t      return tag value in current directory
    TIFFVSetField          setfield.3t      set a tag's value in the current directory
    TIFFWarning            warning.3t       library warning handler
    TIFFWriteDirectory     writedir.3t      write the current directory
    TIFFWriteEncodedStrip  wrestrip.3t      compress and write a strip of data
    TIFFWriteEncodedTile   wretile.3t       compress and write a tile of data
    TIFFWriteRawStrip      wrrstrip.3t      write a raw strip of data
    TIFFWriteRawTile       wrrtile.3t       write a raw tile of data
    TIFFWriteScanline      writeline.3t     write a scanline of data
    TIFFWriteTile          wrrtile.3t       compress and write a tile of data

## TAG USAGE

The table below lists the TIFF tags that are recognized and handled by the library. If no use is indicated in the table, then the library reads and writes the tag, but does not use it internally. Note that some tags are meaningful only when a particular compression scheme is being used; e.g. Group3Options is only useful if Compression is set to CCITT Group 3 encoding. Tags of this sort are considered codec-specific tags and the library does not recognize them except when the Compression tag has been previously set to the relevant compression scheme.

    Tag Name                Value  R/W  Library Use/Notes

    Artist                  315    R/W
    BadFaxLines             326    R/W
    BitsPerSample           258    R/W  lots
    CellLength              265         parsed but ignored
    CellWidth               264         parsed but ignored
    CleanFaxData            327    R/W
    ColorMap                320    R/W
    ColorResponseUnit       300         parsed but ignored
    Compression             259    R/W  choosing codec
    ConsecutiveBadFaxLines  328    R/W
    DataType                32996  R    obsoleted by SampleFormat tag
    DateTime                306    R/W
    DocumentName            269    R/W
    DotRange                336    R/W
    ExtraSamples            338    R/W  lots
    FaxRecvParams           34908  R/W
    FaxSubAddress           34909  R/W
    FaxRecvTime             34910  R/W
    FillOrder               266    R/W  control bit order
    FreeByteCounts          289         parsed but ignored
    FreeOffsets             288         parsed but ignored
    GrayResponseCurve       291         parsed but ignored
    GrayResponseUnit        290         parsed but ignored
    Group3Options           292    R/W  used by Group 3 codec
    Group4Options           293    R/W
    HostComputer            316    R/W
    ImageDepth              32997  R/W  tile/strip calculations
    ImageDescription        270    R/W
    ImageLength             257    R/W  lots
    ImageWidth              256    R/W  lots
    InkNames                333    R/W
    InkSet                  332    R/W
    JPEGTables              347    R/W  used by JPEG codec
    Make                    271    R/W
    Matteing                32995  R    obsoleted by ExtraSamples tag
    MaxSampleValue          281    R/W
    MinSampleValue          280    R/W
    Model                   272    R/W
    NewSubFileType          254    R/W  called SubFileType in spec
    NumberOfInks            334    R/W
    Orientation             274    R/W
    PageName                285    R/W
    PageNumber              297    R/W
    PhotometricInterpretation      262  R/Wused by Group 3 and JPEG codecs
    PlanarConfiguration     284    R/W  data i/o
    Predictor               317    R/W  used by LZW and Deflate codecs
    PrimaryChromacities     319    R/W
    ReferenceBlackWhite     532    R/W
    ResolutionUnit          296    R/W  used by Group 3 codec
    RowsPerStrip            278    R/W  data i/o
    SampleFormat            339    R/W
    SamplesPerPixel         277    R/W  lots
    SMinSampleValue         340    R/W
    SMaxSampleValue         341    R/W
    Software                305    R/W
    StoNits                 37439  R/W
    StripByteCounts         279    R/W  data i/o
    StripOffsets            273    R/W  data i/o
    SubFileType             255    R/W  called OSubFileType in spec
    TargetPrinter           337    R/W
    Thresholding            263    R/W
    TileByteCounts          324    R/W  data i/o
    TileDepth               32998  R/W  tile/strip calculations
    TileLength              323    R/W  data i/o
    TileOffsets             324    R/W  data i/o
    TileWidth               322    R/W  data i/o
    TransferFunction        301    R/W
    WhitePoint              318    R/W
    XPosition               286    R/W
    XResolution             282    R/W
    YCbCrCoefficients       529    R/W  used by TIFFRGBAImage support
    YCbCrPositioning        531    R/W  tile/strip size calulcations
    YCbCrSubsampling        530    R/W
    YPosition               286    R/W
    YResolution             283    R/W  used by Group 3 codec

## PSEUDO TAGS

In addition to the normal TIFF tags the library supports a collection of tags whose values lie in a range outside the valid range of TIFF tags. These tags are termed pseud-tags and are used to control various codec-specific functions within the library. The table below summarizes the defined pseudo-tags.

    Tag Name                Codec  R/W  Library Use/Notes

    TIFFTAG_FAXMODE         G3     R/W  general codec operation
    TIFFTAG_FAXFILLFUNC     G3/G4  R/W  bitmap fill function
    TIFFTAG_JPEGQUALITY     JPEG   R/W  compression quality control
    TIFFTAG_JPEGCOLORMODE   JPEG   R/W  control colorspace conversions
    TIFFTAG_JPEGTABLESMODE  JPEG   R/W  control contents of JPEGTables tag
    TIFFTAG_ZIPQUALITY      Deflate     R/Wcompression quality level
    TIFFTAG_PIXARLOGDATAFMT PixarLog    R/Wuser data format
    TIFFTAG_PIXARLOGQUALITY PixarLog    R/Wcompression quality level
    TIFFTAG_SGILOGDATAFMT   SGILog R/W  user data format

TIFFTAG_FAXMODE
  Control the operation of the Group 3 codec. Possible values (independent bits that can be combined by or'ing them together) are: FAXMODE_CLASSIC (enable old-style format in which the RTC is written at the end of the last strip), FAXMODE_NORTC (opposite of FAXMODE_CLASSIC; also called FAXMODE_CLASSF), FAXMODE_NOEOL (do not write EOL codes at the start of each row of data), FAXMODE_BYTEALIGN (align each encoded row to an 8-bit boundary), FAXMODE_WORDALIGN (align each encoded row to an 16-bit boundary), The default value is dependent on the compression scheme; this pseudo-tag is used by the various G3 and G4 codecs to share code.
TIFFTAG_FAXFILLFUNC
  Control the function used to convert arrays of black and white runs to packed bit arrays. This hook can be used to image decoded scanlines in multi-bit depth rasters (e.g. for display in colormap mode) or for other purposes. The default value is a pointer to a builtin function that images packed bilevel data.
TIFFTAG_IPTCNEWSPHOTO
  Tag contaings image metadata per the IPTC newsphoto spec: Headline, captioning, credit, etc... Used by most wire services.
TIFFTAG_PHOTOSHOP
  Tag contains Photoshop captioning information and metadata. Photoshop uses in parallel and redundantly alongside IPTCNEWSPHOTO information.
TIFFTAG_JPEGQUALITY
  Control the compression quality level used in the baseline algorithm. Note that quality levels are in the range 0-100 with a default value of 75.
TIFFTAG_JPEGCOLORMODE
  Control whether or not conversion is done between RGB and YCbCr colorspaces. Possible values are: JPEGCOLORMODE_RAW (do not convert), and JPEGCOLORMODE_RGB (convert to/from RGB) The default value is JPEGCOLORMODE_RAW.
TIFFTAG_JPEGTABLESMODE
  Control the information written in the JPEGTables tag. Possible values (independent bits that can be combined by or'ing them together) are: JPEGTABLESMODE_QUANT (include quantization tables), and JPEGTABLESMODE_HUFF (include Huffman encoding tables). The default value is JPEGTABLESMODE_QUANT|JPEGTABLESMODE_HUFF.
TIFFTAG_ZIPQUALITY
  Control the compression technique used by the Deflate codec. Quality levels are in the range 1-9 with larger numbers yielding better compression at the cost of more computation. The default quality level is 6 which yields a good time-space tradeoff.
TIFFTAG_PIXARLOGDATAFMT
  Control the format of user data passed in to the PixarLog codec when encoding and passed out from when decoding. Possible values are: PIXARLOGDATAFMT_8BIT for 8-bit unsigned pixels, PIXARLOGDATAFMT_8BITABGR for 8-bit unsigned ABGR-ordered pixels, PIXARLOGDATAFMT_11BITLOG for 11-bit log-encoded raw data, PIXARLOGDATAFMT_12BITPICIO for 12-bit PICIO-compatible data, PIXARLOGDATAFMT_16BIT for 16-bit signed samples, and PIXARLOGDATAFMT_FLOAT for 32-bit IEEE floating point samples.
TIFFTAG_PIXARLOGQUALITY
  Control the compression technique used by the PixarLog codec. This value is treated identically to TIFFTAG_ZIPQUALITY; see the above description.
TIFFTAG_SGILOGDATAFMT
  Control the format of client data passed in to the SGILog codec when encoding and passed out from when decoding. Possible values are: SGILOGDATAFMT_FLTXYZ for converting between LogLuv and 32-bit IEEE floating valued XYZ pixels, SGILOGDATAFMT_16BITLUV for 16-bit encoded Luv pixels, SGILOGDATAFMT_32BITRAW and SGILOGDATAFMT_24BITRAW for no conversion of data, SGILOGDATAFMT_8BITRGB for returning 8-bit RGB data (valid only when decoding LogLuv-encoded data), SGILOGDATAFMT_FLTY for converting between LogL and 32-bit IEEE floating valued Y pixels, SGILOGDATAFMT_16BITL for 16-bit encoded L pixels, and SGILOGDATAFMT_8BITGRY for returning 8-bit greyscale data (valid only when decoding LogL-encoded data).

## DIAGNOSTICS

All error messages are directed through the TIFFError routine. By default messages are directed to stderr in the form: module: message\n. Warning messages are likewise directed through the TIFFWarning routine.

## SEE ALSO

fax2tiff(1), gif2tiff(1), pal2rgb(1), ppm2tiff(1), rgb2ycbcr(1), ras2tiff(1), sgi2tiff(1), tiff2bw(1), tiffdither(1), tiffdump(1), tiffcp(1), tiffcmp(1), tiffgt(1), tiffinfo(1), tiffmedian(1), tiffsplit(1), tiffsv(1),

Tag Image File Format Specification - Revision 6.0, an Aldus Technical Memorandum.

The Spirit of TIFF Class F, an appendix to the TIFF 5.0 specification prepared by Cygnet Technologies.

## BUGS

The library does not support multi-sample images where some samples have different bits/sample.

The library does not support random access to compressed data that is organized with more than one row per tile or strip. The library discards unknown tags. The library should do more validity checking of a directory's contents.

## Index

NAME
SYNOPSIS
DESCRIPTION
DATA TYPES
LIST OF ROUTINES
TAG USAGE
PSEUDO TAGS
DIAGNOSTICS
SEE ALSO
BUGS

This document was created by man2html, using the manual pages.
Time: 01:31:39 GMT, November 23, 1999