# NAME

reference - MRTG 2.10.11 configuration reference

# OVERVIEW

The runtime behaviour of MRTG is governed by a configuration file. Run-of- ther-mill configuration files can be generated with cfgmaker. (Check the cfgmaker manpage). But for more elaborate configurations some hand-tuning is required.

This document describes all the configuration options understood by the mrtg software.

# SYNTAX

MRTG configuration file syntax follows some simple rules:

Keywords must start at the beginning of a line.

Lines which follow a keyword line which start with a blank are appended to the keyword line

Empty Lines are ignored

Lines starting with a # sign are comments.

You can add other files into the configuration file using

Include: file

Example:

     Include: base-options.inc

If included files are specified with relative paths, both the current working directory and the directory containing the main config file will be searched for the files.

# GLOBAL KEYWORDS

## WorkDir

WorkDir specifies where the logfiles and the webpages should be created.

Example:

     WorkDir: /usr/tardis/pub/www/stats/mrtg

# OPTIONAL GLOBAL KEYWORDS

## HtmlDir

HtmlDir specifies the directory where the html (or shtml, but we'll get on to those later) lives.

NOTE: Workdir overrides the settings for htmldir, imagedir and logdir.

Example:

     Htmldir: /www/mrtg/

## ImageDir

ImageDir specifies the directory where the images live. They should be under the html directory.

Example:

     Imagedir: /www/mrtg/images

## LogDir

LogDir specifies the directory where the logs are stored. This need not be under htmldir directive.

Example:

     Logdir: /www/mrtg/logs

## Forks (UNIX only)

With system that supports fork (UNIX for example), mrtg can fork itself into multiple instances while it is acquiring data via snmp.

For situations with high latency or a great number of devices this will speed things up considerably. It will not make things faster, though, if you query a single switch sitting next door.

As far as I know NT can not fork so this option is not available on NT.

Example:

     Forks: 4

## EnableIPv6

When set to yes, IPv6 support is enabled if the required libraries are present (see the mrtg-ipv6 manpage). When IPv6 is enabled, mrtg can talk to routers using SNMP over IPv6 and targets may be specified by their numeric IPv6 addresses as well as by hostname or IPv4 address.

If IPv6 is enabled and the target is a hostname, mrtg will try to resolve the hostname to an IPv6 address and, if this fails, to an IPv4 address. Note that mrtg will only use IPv4 if you specify an IPv4 address or a hostname with no corresponding IPv6 address; it will not fall back to IPv4 if it simply fails to communicate with the target using IPv6. This is by design.

Note that many routers do not currently support SNMP over IPv6. Use the IPv4Only per target option for these routers.

IPv6 is disabled by default.

Example:

     EnableIPv6: Yes

## Refresh

How many seconds apart should the browser (Netscape) be instructed to reload the page? If this is not defined, the default is 300 seconds (5 minutes).

Example:

     Refresh: 600

## Interval

How often do you call mrtg? The default is 5 minutes. If you call it less often, you should specify it here. This does two things:

The generated HTML page contains the right information about the calling interval ...

A META header in the generated HTML page will instruct caches about the time-to-live of this page .....

In this example, we tell mrtg that we will be calling it every 10 minutes. If you are calling mrtg every 5 minutes, you can leave this line commented out.

Example:

     Interval: 10

Note that unless you are using rrdtool you can not set Interval to less than 5 minutes. If you are using rrdtool you can set interval down to 1 minute. Note though, setting the Interval for an rrdtool/mrtg setup will influence the initial creation of the database. If you change the interval later, all existing databases will remain at the resolution they were initially created with.

## WriteExpires

With this switch mrtg will generate .meta files for CERN and Apache servers which contain Expiration tags for the html and gif files. The *.meta files will be created in the same directory as the other files, so you will have to set ``MetaDir .'' and ``MetaFiles on'' in your apache.conf or .htaccess file for this to work

NOTE: If you are running Apache-1.2 or later, you can use the mod_expire to achieve the same effect ... see the file htaccess.txt

Example:

     WriteExpires: Yes

## NoMib2

Normally we ask the SNMP device for 'sysUptime' and 'sysName' properties. Some do not have these. If you want to avoid getting complaints from mrtg about these missing properties, specify the nomib2 option.

An example of agents which do not implement base mib2 attributes are Computer Associates - Unicenter TNG Agents. CA relies on using the base OS SNMP agent in addition to its own agents to supplement the management of a system.

Example:

     NoMib2: Yes

## SingleRequest

Some SNMP implementations can not deal with requests asking for multiple snmp variables in one go. Set this in your cfg file to force mrtg to only ask for one variable per request.

Examples

     SingleRequest: Yes

## SnmpOptions

Apart from the per target timeout options, you can also configure the behaviour of the snmpget process on a more profound level. SnmpOptions accepts a hash of options. The following options are currently supported:

     timeout                   => $default_timeout,
     retries                   => $default_retries,
     backoff                   => $default_backoff,
     default_max_repetitions   => $max_repetitions,
     lenient_source_port_matching => 0,
     lenient_source_address_matching => 1

The values behind the options indicate the current default value. Note that these settings OVERRIDE the per target timeout settings.

Example:

     SnmpOptions: retries => 2, only_ip_address_matching => 0

Note that AS/400 snmp seems to be broken in a way which prevents mrtg from working with it unless

     SnmpOptions: lenient_source_port_matching => 1

is set.

## IconDir

If you want to keep the mrtg icons in someplace other than the working (or imagedir) directory, use the IconDir variable for defining the url of the icons directory.

Example:

     IconDir: /mrtgicons/

## LoadMIBs

Load the MIB `file(s)` specified and make its OIDs available as symbolic names. For better efficiancy, a cache of MIBs is maintained in the WorkDir.

Example:

     LoadMIBs: /dept/net/mibs/netapp.mib,/usr/local/lib/ft100m.mib

## Language

Switch output format to the selected Language (Check the translate directory to see which languages are supported at the moment. In this directory you can also find instructions on how to create new translations).

Currently the following laguages are supported:

big5 brazilian bulgarian catalan chinese croatian czech danish dutch eucjp french galician gb gb2312 german greek hungarian icelandic indonesia iso2022jp italian korean lithuanian malay norwegian polish portuguese romanian russian russian1251 serbian slovak slovenian spanish swedish turkish ukrainian

Example:

     Language: danish

## LogFormat

Setting LogFormat to 'rrdtool' in your mrtg.cfg file enables rrdtool mode. In rrdtool mode, mrtg relies on rrdtool to do its logging. Graphs and html pages will be generated on the fly by the 14all.cgi which can be found in the contrib section together with a short readme ... This feature has been contributed by Rainer Bawidamann <bawidama@users.sourceforge.net>. Please check his website for more information: http://www.wh-hms.uni-ulm.de/~widi/14all/

Example:

     LogFormat: rrdtool

## LibAdd

If you are using rrdtool mode and your rrdtool Perl module (RRDs.pm) is not installed in a location where perl can find it on its own, you can use LibAdd to supply an appropriate path.

Example:

     LibAdd: /usr/local/rrdtool/lib/perl/

## PathAdd

If the rrdtool executable can not be found in the normal `PATH`, you can use this keyword to add a suitable directory to your path.

Example:

     PathAdd: /usr/local/rrdtool/bin/

## RunAsDaemon

The RunAsDaemon keyword enables daemon mode operation. The purpose of daemon mode is that MRTG is launched once and not repeatedly (as it is with cron). This behavior saves computing resourses as loading and parsing of configuration files happens only once.

Using daemon mode MRTG itself is responible for timing the measurement intervals. Therfore its important to set the Interval keyword to an apropiate value.

Note that when using daemon mode MRTG should no longer be started from cron as each new process runs forever. Instead MRTG should be started from the command prompt or by a system startup script.

If you want mrtg to run under a particular user and group (it is not recomended to run MRTG as root) then you can use the --user=user_name and --group=group_name options on the mrtg commandline.

     mrtg --user=mrtg_user --group=mrtg_group mrtg.cfg

Also note that in daemon mode restarting the process is required in order to activate changes in the config file.

Under UNIX, the Daemon switch causes mrtg to fork into background after checking its config file. On Windows NT the MRTG process will detach from the console, but because the NT/2000 shell waits for its children you have to use this special start sequence when you launch the program:

     start /b perl mrtg mrtg.cfg

You may have to add path information equal to what you add when you run mrtg from the commandline.

Example

     RunAsDaemon:Yes
     Interval:5

This makes MRTG run as a daemon beginning data collection every 5 minutes

## ConversionCode

Some devices may produce non-numeric values that would nevertheless be useful to graph with MRTG if those values could be converted to numbers. The ConversionCode keyword specifies the path to a file containing Perl code to perform such conversions. The code in this file must consist of one or more Perl subroutines. Each subroutine must accept a single string argument and return a single numeric value. When RRDtool is in use, a decimal value may be returned. When the name of one of these subroutines is specified in a target definition (see below), MRTG calls it twice for that target, once to convert the the input value being monitored and a second time to convert the output value. The subroutine must return an undefined value if the conversion fails. In case of failure, a warning may be posted to the MRTG log file using Perl's warn function. MRTG imports the subroutines into a separate name space (package MRTGConversion), so the user need not worry about pollution of MRTG's global name space. MRTG automatically prepends this package declaration to the user-supplied code.

Example: Suppose a particular OID returns a character string whose length is proportional to the value to be monitored. To convert this string to a number that can be graphed by MRTG, create a file arbitrarily named ``MyConversions.pl'' containing the following code:

     # Return the length of the string argument
     sub Length2Int {
       my $value = shift;
       return length( $value );
     }

Then include the following global keyword in the MRTG configuration file (assuming that the conversion code file is saved in the mrtg/bin directory along with mrtg itself):

     ConversionCode: MyConversions.pl

This will cause MRTG to include the definition of the subroutine Length2Int in its execution environment. Length2Int can then be invoked on any target by appending ``|Length2Int'' to the target definition as follows:

     Target[ezwf]: 1.3.6.1.4.1.999.1&1.3.6.1.4.1.999.1:public@mydevice|Length2Int

See ``Extended Host Name Syntax'' below for complete target definition syntax information.

# PER TARGET CONFIGURATION

Each monitoring target must be identified by a unique name. This name must be appended to each parameter belonging to the same target. The name will also be used for naming the generated webpages, logfiles and images for this target.

## Target

With the Target keyword you tell mrtg what it should monitor. The Target keyword takes arguments in a wide range of formats:

Basic
  The most basic format is ``port:community@router'' This will generate a traffic graph for the interface 'port' of the host 'router' (dns name or IP address) and it will use the community 'community' (snmp password) for the snmp query.

  Example:

       Target[ezwf]: 2:public@wellfleet-fddi.ethz.ch

  If your community contains a ``@'' or a `` '' these characters must be escaped with a ``\''.

       Target[bla]: 2:stu\ pi\@d@router

SNMPv2c
  If you have a fast router you might want to try to poll the ifHC* counters. This feature gets activated by switching to SNMPv2c. Unfortunately not all devices support SNMPv2c yet. If it works, this will prevent your counters from wraping within the 5 minute polling interval, since we now use 64 bit instead of the normal 32 bit.

  Example:

       Target[ezwf]: 2:public@router1:::::2

Reversing
  Sometimes you are sitting on the wrong side of the link, and you would like to have mrtg report Incoming traffic as Outgoing and vice versa. This can be achieved by adding the '-' sign in front of the ``Target'' description. It flips the incoming and outgoing traffic rates.

  Example:

       Target[ezci]: -1:public@ezci-ether.ethz.ch

Explicit OIDs
  You can also explicitly define which OID to query by using the following syntax 'OID_1&OID_2:community@router' The following example will retrieve error counts for input and output on interface 1. MRTG needs to graph two variables, so you need to specify two OID's such as temperature and humidity or error input and error output.

  Example:

       Target[ezwf]: 1.3.6.1.2.1.2.2.1.14.1&1.3.6.1.2.1.2.2.1.20.1:public@myrouter

MIB Variables
  MRTG knows a number of symbolic SNMP variable names. See the file mibhelp.txt for a list of known names. One example are the ifInErrors and ifOutErrors. This means you can specify the above as:

  Example:

       Target[ezwf]: ifInErrors.1&ifOutErrors.1:public@myrouter

Interface by IP
  Sometimes SNMP interface index can change, like when new interfaces are added or removed. This can cause all Target entries in your config file to become offset, causing MRTG to graphs wrong instances etc. MRTG supports IP address instead of ifindex in target definition. Then MRTG will query snmp device and try to map IP address to the current ifindex. You can use IP addresses in every type of target definition by adding IP address of the numbered interface after OID and separation char '/'.

  Make sure that the given IP address is used on your same target router, especially when graphing two different OIDs and/or interface split by '&' delimiter.

  You can tell cfgmaker to generate such references with the option --ifref=ip.

  Example:

       Target[ezwf]: /1.2.3.4:public@wellfleet-fddi.ethz.ch
       Target[ezci]: -/1.2.3.4:public@ezci-ether.ethz.ch
       Target[ezwf]: 1.3.6.1.2.1.2.2.1.14/1.2.3.4&1.3.6.1.2.1.2.2.1.14/1.2.3.4:public@myrouter
       Target[ezwf]: ifInErrors/1.2.3.4&ifOutErrors/1.2.3.4:public@myrouter

Interface by Description
  If you can not use IP addresses you might want to use the interface names. This works similar to the IP address aproach except that the prefix to use is a \ instead of a /

  You can tell cfgmaker to generate such references with the option --ifref=descr.

  Example:

       Target[ezwf]: \My-Interface2:public@wellfleet-fddi.ethz.ch
       Target[ezci]: -\My-Interface2:public@ezci-ether.ethz.ch
       Target[ezwf]: 1.3.6.1.2.1.2.2.1.14\My-Interface2&1.3.6.1.2.1.2.2.1.14\My-Interface3:public@myrouter
       Target[ezwf]: ifInErrors\My-Interface2&ifOutErrors\My-Interface3:public@myrouter

  If your description contains a ``&'', a ``:'', a ``@'' or a `` '' you can include them but you must escape with a backlash:

       Target[ezwf]: \fun\:\ ney\&ddd:public@hello.router

Interface by Name
  This is the only sensible way to reference the interfaces of your switches.

  You can tell cfgmaker to generate such references with the option --ifref=name.

  Example:

       Target[ezwf]: #2/11:public@wellfleet-fddi.ethz.ch
       Target[ezci]: -#2/11:public@ezci-ether.ethz.ch
       Target[ezwf]: 1.3.6.1.2.1.2.2.1.14#3/7&1.3.6.1.2.1.2.2.1.14#3/7:public@myrouter
       Target[ezwf]: ifInErrors#3/7&ifOutErrors#3/7:public@myrouter

  If your description contains a ``&'', a ``:'', a ``@'' or a `` '' you can include them but you must escape with a backlash:

       Target[ezwf]: #\:\ fun:public@hello.router

  <Note that the # sign will be interpreted as a comment character if it is the first non white-space character on the line.>

Interface by Ethernet Address
  When the SNMP interface index changes, you can key that interface by its 'Physical Address', sometimes called a 'hard address', which is the SNMP variable 'ifPhysAddress'. Internally, MRTG matches the Physical Address from the *.cfg file to its current index, and then uses that index for the rest of the session.

  You can use the Physical Address in every type of target definition by adding the Physical Address after the OID and the separation char '!' (analogous to the IP address option). The Physical address is specified as '-' delimited octets, such as ``0a-0-f1-5-23-18'' (omit the double quotes). Note that some routers use the same Hardware Ethernet Address for all of their Interfaces which prevents unique interface identification. Mrtg will notice such problems and alert you.

  You can tell cfgmaker to generate configuration files with hardware ethernet address references by using the option --ifref=eth.

  Example:

       Target[ezwf]: !0a-0b-0c-0d:public@wellfleet-fddi.ethz.ch
       Target[ezci]: -!0-f-bb-05-71-22:public@ezci-ether.ethz.ch
       Target[ezwf]: 1.3.6.1.2.1.2.2.1.14!0a-00-10-23-44-51&!0a-00-10-23-44-51:public@myrouter
       Target[ezwf]: ifInErrors!0a-00-10-23-44-51&ifOutErrors!0a-00-10-23-44-51:public@myrouter

Interface by Type
  It seems that there are devices that try to defy all monitoring efforts: the interesting interfaces have neither ifName nor a constant ifDescr not to mention a persistant ifIndex. The only way to get a constant mapping is by looking at the interface type, because the interface you are interested in is unique in the device you are looking at ...

  You can tell cfgmaker to generate such references with the option --ifref=type.

  Example:

       Target[ezwf]: %13:public@wellfleet-fddi.ethz.ch
       Target[ezci]: -%13:public@ezci-ether.ethz.ch
       Target[ezwf]: 1.3.6.1.2.1.2.2.1.14%13&1.3.6.1.2.1.2.2.1.14%14:public@myrouter
       Target[ezwf]: ifInErrors%13&ifOutErrors%14:public@myrouter

Extended Host Name Syntax
  In all places where ``community@router'' is accepted, you can add additional parameters for the SNMP communication using colon-separated suffixes. You can also append a pipe symbol ( | ) and the name of a numeric conversion subroutine as described under the global keyword ``ConversionCode'' above. The full syntax is as follows:

       community@router[:[port][:[timeout][:[retries][:[backoff][:[version]][|name]]]]]

  where the meaning of each parameter is as follows:

port
  the UDP port under which to contact the SNMP agent (default: 161)

timeout
  initial timeout for SNMP queries, in seconds (default: 2.0)

retries
  number of times a timed-out request will be retried (default: 5)

backoff
  factor by which the timeout is multiplied on every retry (default: 1.0).

version
  for SNMP version. If you have a fast router you might want to put a '2' here. This will make mrtg try to poll the 64 bit counters and thus prevent excessive counter wrapping. Not all routers support this though.

  Example:

       3:public@router1:::::2

name
  the name of the subroutine that MRTG will call to convert the input and output values to integers. See the complete example under the global keyword ``ConversionCode'' above.

  Example:

       1.3.6.1.4.1.999.1&1.3.6.1.4.1.999.2:public@mydevice:161::::2|Length2Int

  This would retrieve values from the OID 1.3.6.1.4.1.999.1 for input and .2 for output on mydevice using UDP port 161 and SNMP version 2, and would execute the user-defined numeric conversion subroutine Length2Int to convert those values to integers.

A value that equals the default value can be omitted. Trailing colons can be omitted, too. The pipe symbol followed by the name parameter, if present, must come at the end. There must be no spaces around the colons or pipe symbol.

Example:

      Target[ezci]: 1:public@ezci-ether.ethz.ch:9161::4

This would refer to the input/output octet counters for the interface with ifIndex 1 on ezci-ether.ethz.ch, as known by the SNMP agent listening on UDP port 9161. The standard initial timeout (2.0 seconds) is used, but the number of retries is set to four. The backoff value is the default.

Numeric IPv6 addresses
  If IPv6 is enabled you may also specify a target using its IPv6 address. To avoid ambiguity with the port number, numeric IPv6 addresses must be placed in square brackets.

  Example:

       Target[IPv6test]: 2:public@[2001:760:4::]:6161::4

External Monitoring Scripts
  If you want to monitor something which does not provide data via snmp you can use some external program to do the data gathering.

  The external command must return 4 lines of output:

Line 1
  current state of the first variable, normally 'incoming bytes count'

Line 2
  current state of the second variable, normally 'outgoing bytes count'

Line 3
  string (in any human readable format), telling the uptime of the target.

Line 4
  string, telling the name of the target.

Depending on the type of data your script returns you might want to use the 'gauge' or 'absolute' arguments for the Options keyword.

Example:

     Target[ezwf]: `/usr/local/bin/df2mrtg /dev/dsk/c0t2d0s0`

Note the use of the backticks (`), not apostrophes (') around the command.

If you want to use a backtick in the command name this can be done but you must escape it with a backslash ...

If your script does not have any data to return but does not want mrtg to complain about invalid data, it can return 'UNKNOWN' instead of a number. Note though that only rrdtool is realy equipped to handle unknown data well.

Multi Target Syntax
  You can also combine several target definitions in a mathematical expression. Any syntactically correct expression that the Perl interpreter can evaluate to will work. An expression could be used, for example, to aggregate both B channels in an ISDN connection or to calculate the percentage hard disk utilization of a server from the absolute used space and total capacity.

  Examples:

       Target[ezwf]: 2:public@wellfleetA + 1:public@wellfleetA

       Target[ezwf]: 1.3.6.1.4.1.999.1&1.3.6.1.4.1.999.2:public@mydevice /
           1.3.6.1.4.1.999.3&1.3.6.1.4.1.999.4:public@mydevice * 100

  Note that whitespace must surround each target definition in the expression. Target definitions themselves must not contain whitespace, except in interface descriptions and interface names, where each whitespace character is escaped by a backslash.

  MRTG automatically rounds the result of the expression to an integer unless RRDTool logging is in use and the gauge option is in effect for the target. Internally MRTG uses Perl's Math::BigFloat package to calculate the result of the expression with 40 digits of precision. Even in extreme cases, where, for example, you take the difference of two 64-bit integers, the result of the expression should be accurate.

SNMP Request Optimization
  MRTG is designed to economize on its SNMP requests. Where a target definition appears more than once in the configuration file, MRTG requests the data from the device only once per round of data collection and uses the collected data for each instance of a particular target. Recognition of two target definitions as being identical is based on a simple string match rather than any kind of deeper semantic analysis.

  Example:

       Target[Targ1]: 1:public@CiscoA
       Target[Targ2]: 2:public@CiscoA
       Target[Targ3]: 1:public@CiscoA + 2:public@CiscoA
       Target[Targ4]: 1:public@CISCOA

  This results in a total of three SNMP requests. Data for 1:public@CiscoA and 2:public@CiscoA are requested only once each, and used for Targ1, Targ2, and Targ3. Targ4 causes another SNMP request for 1:public@CISCOA, which is not recognized as being identical to 1:public@CiscoA.

## MaxBytes

The maximum value either of the two variables monitored are allowed to reach. For monitoring router traffic this is normally the bytes per second this interface port can carry.

If a number higher than MaxBytes is returned, it is ignored. Also read the section on AbsMax for further info. The MaxBytes value is also used in calculating the Y range for unscaled graphs (see the section on Unscaled).

Since most links are rated in bits per second, you need to divide their maximum bandwidth (in bits) by eight (8) in order to get bytes per second. This is very important to make your unscaled graphs display realistic information. T1 = 193000, 56K = 7000, Ethernet = 1250000. The MaxBytes value will be used by mrtg to decide whether it got a valid response from the router.

If you need two different MaxBytes values for the two monitored variables, you can use MaxBytes1 and MaxBytes2 instead of MaxBytes.

Example:

     MaxBytes[ezwf]: 1250000

## Title

Title for the HTML page which gets generated for the graph.

Example:

     Title[ezwf]: Traffic Analysis for Our Nice Company

# OPTIONAL PER TARGET KEYWORDS

## PageTop

Things to add to the top of the generated HTML page. Note that you can have several lines of text as long as the first column is empty.

Note that the continuation lines will all end up on the same line in the html page. If you want linebreaks in the generated html use the '\n' sequence.

Example:

     PageTop[ezwf]: <H1>Traffic Analysis for ETZ C95.1</H1>
       Our Campus Backbone runs over an FDDI line\n
       with a maximum transfer rate of 12.5 megabytes per
       Second.

## RouterUptime

In cases where you calculate the used bandwidth from several interfaces you normaly don't get the router uptime and router name displayed on the web page.

If these interfaces are on the same router and the uptime and name should be displayed you have to specify its community and address again with the RouterUptime keyword.

Example:

     Target[kacisco.comp.edu]: 1:public@194.64.66.250 + 2:public@194.64.66.250
     RouterUptime[kacisco.comp.edu]: public@194.64.66.250

## RouterName

If the default name of the router is incorrect/uninformative, you can use RouterName to specify a different OID on either the same or a different host.

A practical example: sysName on BayTech DS72 units always display ``ds72'', no matter what you set the Unit ID to be. Instead, the Unit ID is stored at 1.3.6.1.4.1.4779.1.1.3.0, so we can have MRTG display this instead of sysName.

Example:

     RouterName[kacisco.comp.edu]: 1.3.6.1.4.1.4779.1.1.3.0

A different OID on a different host can also be specified:

     RouterName[kacisco.comp.edu]: 1.3.6.1.4.1.4779.1.1.3.0:public@194.64.66.251

## MaxBytes1

Same as MaxBytes, for variable 1.

## MaxBytes2

Same as MaxBytes, for variable 2.

## IPv4Only

Many IPv6 routers do not currently support SNMP over IPv6 and must be monitored using IPv4. The IPv4Only option forces mrtg to use IPv4 when communicating with the target, even if IPv6 is enabled. This is useful if the target is a hostname with both IPv4 and IPv6 addresses; without the IPv4Only keyword, monitoring such a router will not work if IPv6 is enabled.

If set to no (the default), mrtg will use IPv6 unless the target has no IPv6 addresses, in which case it will use IPv4. If set to yes, mrtg will only use IPv4.

Note that if this option is set to yes and the target does not have an IPv4 address, communication with the target will fail.

This option has no effect if IPv6 is not enabled.

Example:

     Target[v4onlyrouter_1]: 1:public@v4onlyrouter
     IPv4Only[v4onlyrouter_1]: Yes

## PageFoot

Things to add to the bottom of the generated HTML page. Note that you can have several lines of text as long as the first column is empty.

Note that the continuation lines will all end up on the same line in the html page. If you want linebreaks in the generated html use the '\n' sequence.

The material will be added just before the </BODY> tag:

Example:

     PageFoot[ezwf]: Contact <A HREF="mailto:peter@x.yz">Peter</A>;
      if you have questions regarding this page

## AddHead

Use this tag like the PageTop header, but its contents will be added between </TITLE> and </HEAD>.

Example:

     AddHead[ezwf]: <link rev="made" href="mailto:mrtg@blabla.edu">;

## BodyTag

BodyTag lets you supply your very own <body ...> tag for the generated webpages.

Example:

     BodyTag[ezwf]: <BODY LEFTMARGIN="1" TOPMARGIN="1"
                          BACKGROUND="/stats/images/bg.neo2.gif">

## AbsMax

If you are monitoring a link which can handle more traffic than the MaxBytes value. Eg, a line which uses compression or some frame relay link, you can use the AbsMax keyword to give the absolute maximum value ever to be reached. We need to know this in order to sort out unrealistic values returned by the routers. If you do not set AbsMax, rateup will ignore values higher than MaxBytes.

Example:

     AbsMax[ezwf]: 2500000

## Unscaled

By default each graph is scaled vertically to make the actual data visible even when it is much lower than MaxBytes. With the Unscaled variable you can suppress this. It's argument is a string, containing one letter for each graph you don't want to be scaled: d=day w=week m=month y=year. There is also a special case to unset the variable completely: n=none. This could be useful in the event you need to override a global configuration. In the example scaling for the yearly and the monthly graph are suppressed.

Example:

     Unscaled[ezwf]: ym

## WithPeak

By default the graphs only contain the average values of the monitored variables - normally the transfer rates for incoming and outgoing traffic. The following option instructs mrtg to display the peak 5 minute values in the [w]eekly, [m]onthly and [y]early graph. In the example we define the monthly and the yearly graph to contain peak as well as average values.

Examples:

     WithPeak[ezwf]: ym

## Suppress

By default mrtg produces 4 graphs. With this option you can suppress the generation of selected graphs. The option value syntax is analogous to the above two options. In this example we suppress the yearly graph as it is quite empty in the beginning.

Example:

     Suppress[ezwf]: y

## Extension

By default, mrtg creates .html files. Use this option to tell mrtg to use a different extension. For example you could set the extension to php3, then you will be able to enclose PHP tags into the output (useful for getting a router name out of a database).

Example:

     Extension[ezwf]: phtml

## Directory

By default, mrtg puts all the files that it generates for each target (the GIFs, the HTML page, the log file, etc.) in WorkDir.

If the Directory option is specified, the files are instead put into a directory under WorkDir or Log-, Image- and HtmlDir). (For example the Directory option below would cause all the files for a target ezwf to be put into directory /usr/tardis/pub/www/stats/mrtg/ezwf/ .)

The directory must already exist; mrtg will not create it.

Example:

     WorkDir: /usr/tardis/pub/www/stats/mrtg
     Directory[ezwf]: ezwf

NOTE: the Directory option must always be 'relative' or bad things will happen.

## XSize and YSize

By default mrtgs graphs are 100 by 400 pixels wide (plus some more for the labels. In the example we get almost square graphs ...

Note: XSize must be between 20 and 600; YSize must be larger than 20

Example:

     XSize[ezwf]: 300
     YSize[ezwf]: 300

## XZoom and YZoom

If you want your graphs to have larger pixels, you can ``Zoom'' them.

Example:

     XZoom[ezwf]: 2.0
     YZoom[ezwf]: 2.0

## XScale and YScale

If you want your graphs to be actually scaled use XScale and YScale. (Beware: while this works, the results look ugly (to be frank) so if someone wants to fix this: patches are welcome.

Example:

     XScale[ezwf]: 1.5
     YScale[ezwf]: 1.5

## YTics and YTicsFactor

If you want to show more than 4 lines per graph, use YTics. If you want to scale the value used for the YLegend of these tics, use YTicsFactor. The default value for YTics is 4 and the default value for YTicsFactor is 1.0 .

Example:

Suppose you get values ranging from 0 to 700. You want to plot 7 lines and want to show 0, 1, 2, 3, 4, 5, 6, 7 instead of 0, 100, 200, 300, 400, 500, 600, 700. You should write then:

      YTics[ezwf]: 7
      YTicsFactor[ezwf]: 0.01

## Factor

If you want to multiply all numbers shown below the graph with a constant factor, use this directive to define it ..

Example:

      Factor[as400]: 4096

## Step

Change the default step from 5 * 60 seconds to something else (I have not tested this much ...)

Example:

     Step[ezwf]: 60

## PNGTitle

When using rateup for graph generation, this will print the given title in the graph it generates.

Example:

     PNGTitle[ezwf]: WAN Link UK-US

## Options

The Options Keyword allows you to set some boolean switches:

growright
  The graph grows to the left by default. This option flips the direction of growth causing the current time to be at the right edge of the graph and the history values to the left of it.

bits
  All the monitored variable values are multiplied by 8 (i.e. shown in bits instead of bytes) ... looks much more impressive :-) It also affects the 'factory default' labeling and units for the given target.

perminute
  All the monitored variable values are multiplied by 60 (i.e. shown in units per minute instead of units per second) in case of small values more accurate graphs are displayed. It also affects the 'factory default' labeling and units for the given target.

perhour
  All the monitored variable values are multiplied by 3600 (i.e. shown in units per hour instead of units per second) in case of small values more accurate graphs are displayed. It also affects the 'factory default' labeling and units for the given target.

noinfo
  Suppress the information about uptime and device name in the generated webpage.

nopercent
  Don't print usage percentages.

transparent
  Make the background of the generated gifs transparent.

integer
  Print summary lines below graph as integers without commas.

dorelpercent
  The relative percentage of IN-traffic to OUT-traffic is calculated and displayed in the graph as an additional line. Note: Only a fixed scale is available (from 0 to 100%). Therefore if IN-traffic is greater than OUT-traffic then 100% is displayed. If you suspect that your IN-traffic is not always less than or equal to your OUT-traffic you are urged to not use this options. Note: If you use this option in combination with the Colours options, a fifth colour-name colour-value pair is required there.

avgpeak
  There are some ISPs who use the average Peak values to bill their customers. Using this option MRTG displays these values for each graph. The value is built by averaging the max 5 minute traffic avarage for each 'step' shown in the graph. For the Weekly graph this means that it builds the average of all 2 hour intervals 5 minute peak values. (Confused? Thought so!)

gauge
  Treat the values gathered from target as 'current status' measurements and not as ever incrementing counters. This would be useful to monitor things like disk space, processor load, temperature, and the like ...

  In the absence of 'gauge' or 'absolute' options, MRTG treats variables as a counters and calculates the difference between the current and the previous value and divides that by the elapsed time between the last two readings to get the value to be plotted.

absolute
  This is for counter type data sources which reset their value when they are read. This means that rateup does not have to build the difference between the current and the last value read from the data source. The value obtained is still divided by the elapsed time between the current and the last reading, which makes it different from the 'gauge' option. Useful for external data gatherers.

unknaszero
  Log unknown data as zero instead of the default behaviour of repeating the last value seen. Be careful with this, often a flat line in the graph is much more obvious than a line at 0.

withzeroes
  Normally we ignore all values which are zero when calculating the average transfer rate on a line. If this is not desirable use this option.

noborder
  If you are using rateup to log data, MRTG will create the graph images. Normally these images have a shaded border around them. If you do not want the border to be drawn, enable this option. This option has no effect if you are not using rateup.

noarrow
  As with the option above, this effects rateup graph generation only. Normally rateup will generate graphs with a small arrow showing the direction of the data. If you do not want this arrow to be drawn, enable this option. This option has no effect if you are not using rateup.

noi
  When using rateup for graph generation, you can use this option to stop rateup drawing a graph for the 'I' or first variable. This also removes entries for this variable in the HTML page MRTG generates, and will remove the peaks for this variable if they are enabled. This allows you to hide this data, or can be very useful if you are only graphing one line of data rather than two. This option is not destructive - any data received for the the variable continued to be logged, it just isn't shown.

noo
  Same as above, except relating to the 'O' or second variable.

nobanner
  When using rateup for graph generation, this option disables MRTG adding the MRTG banner to the HTML pages it generates.

nolegend
  When using rateup for graph generation, this option will stop MRTG from creating a legend at the bottom of the HTML pages it generates.

printrouter
  When using rateup for graph generation, this option will print the router name in the graph it generates. This option is overridden by the value of PNGTitle if one is given

pngdate
  When using rateup for graph generation, this option will print a timestamp in the graph it generates, including a timezone if one is specified by the 'Timezone' parameter.

Example:

     Options[ezwf]: growright, bits

## kilo

Use this option to change the multiplier value for building prefixes. Defaultvalue is 1000. This tag is for the special case that 1kB = 1024B, 1MB = 1024kB and so far.

Example:

     kilo[ezwf]: 1024

## kMG

Change the default multiplier prefixes (,k,M,G,T,P). In the tag ShortLegend define only the basic units. Format: Comma seperated list of prefixed. Two consecutive commas or a comma at start or end of the line gives no prefix on this item. Note: If you do not want prefixes, just put two consecutive commas.

Example: velocity in nm/s (nanometers per second) displayed in nm/h.

     ShortLegend[ezwf]: m/h
     kMG[ezwf]: n,u,m,,k,M,G,T,P
     options[ezwf]: perhour

## Colours

The Colours tag allows you to override the default colour scheme. Note: All 4 of the required colours must be specified here. The colour name ('Colourx' below) is the legend name displayed, while the RGB value is the real colour used for the display, both on the graph and in the html doc.

Format is: Col1#RRGGBB,Col2#RRGGBB,Col3#RRGGBB,Col4#RRGGBB

Important: If you use the dorelpercent options tag a fifth colour name colour value pair is required: Col1#RRGGBB,Col2#RRGGBB,Col3#RRGGBB,Col4#RRGGBB,Col5#RRGGBB

Colour1
  First variable (normally Input) on default graph.

Colour2
  Second variable (normally Output) on default graph.

Colour3
  Max first variable (input).

Colour4
  Max second variable (output).

RRGGBB
  2 digit hex values for Red, Green and Blue.

Example:

     Colours[ezwf]: GREEN#00eb0c,BLUE#1000ff,DARK GREEN#006600,VIOLET#ff00ff

## Background

With the Background tag you can configure the background colour of the generated HTML page.

Example:

     Background[ezwf]: #a0a0a0a

## YLegend, ShortLegend, Legend[1234]

The following keywords allow you to override the text displayed for the various legends of the graph and in the HTML document:

YLegend
  The Y-axis label of the graph. Note that a text which is too long to fit in the graph will be silently ignored.

ShortLegend
  The units string (default 'b/s') used for Max, Average and Current

Legend[1234IO]
  The strings for the colour legend.

Example:

      YLegend[ezwf]: Bits per Second
      ShortLegend[ezwf]: b/s
      Legend1[ezwf]: Incoming Traffic in Bits per Second
      Legend2[ezwf]: Outgoing Traffic in Bits per Second
      Legend3[ezwf]: Maximal 5 Minute Incoming Traffic
      Legend4[ezwf]: Maximal 5 Minute Outgoing Traffic
      LegendI[ezwf]: &nbsp;In:
      LegendO[ezwf]: &nbsp;Out:

Note, if LegendI or LegendO are set to an empty string with

     LegendO[ezwf]:

The corresponding line below the graph will not be printed at all.

## Timezone

If you live in an international world, you might want to generate the graphs in different timezones. This is set in the TZ variable. Under certain operating systems like Solaris, this will provoke the localtime call to give the time in the selected timezone.

Example:

     Timezone[ezwf]: Japan

The Timezone is the standard Solaris timezone, ie Japan, Hongkong, GMT, GMT+1 etc etc.

## Weekformat

By default, mrtg (actually rateup) uses the `strftime(3)` '%W' option to format week numbers in the monthly graphs. The exact semantics of this format option vary between systems. If you find that the week numbers are wrong, and your system's `strftime(3)` routine supports it, you can try another format option. The POSIX '%V' option seems to correspond to a widely used week numbering convention. The week format character should be specified as a single letter; either W, V, or U.

Example:

     Weekformat[ezwf]: V

## RRDRowCount

This affects the creation of new rrd files. By default rrds are created to hold about 1 day's worth of high resolution data. (plus 1 week of 30 minute data, 2 months of 2 hour data and 2 years of 1 day data). With this Keyword you can change the number of base interval entries configured for new rrds as they get created. Note that you must take the interval time into account.

Example:

     RRDRowCount[ezwf]: 1600

# THRESHOLD CHECKING

Through its threshold checking functionality mrtg is able to detect threshold problems for the various targets and can call external scripts to handle those problems (e.g. send email or a page to an administrator).

Threshold checking is configured through the following parameters:

## ThreshDir (GLOBAL)

By defining ThreshDir to point to a writable directory, MRTG will only alert you when a threshold boundery has been crossed.

Example:

     ThreshDir: /var/mrtg/thresh

## ThreshMinI (PER TARGET)

This is the minimum acceptable value for the Input (first) parameter. If the parameter falls below this value, the program specified in ThreshProgI will be run. If the value ends in '%' then the threshold is defined relative to MaxBytes.

## ThreshMaxI (PER TARGET)

This is the maximum acceptable value for the Input (first) parameter. If the parameter falls above this value, the program specified in ThreshProgI will be run. If the value ends in '%' then the threshold is defined relative to MaxBytes.

## ThreshDesc (PER TARGET)

Its value will be assigned to the environment variable THRESH_DESC before any of the programs mentioned below are called. The programms can use the value of this variable to produce more user-friendly output.

## ThreshProgI (PER TARGET)

This defines a program to be run if ThreshMinI or ThreshMaxI is broken. MRTG passes 3 arguments: the $router variable, the threshold value broken, and the current parameter value.

## ThreshProgOKI (PER TARGET)

This defines a program to be run if the parameter is currently OK (based on ThreshMinI and ThreshMaxI), but wasn't OK on the previous running -- based on the files found in ThreshDir. MRTG passes 3 arguments: the $router variable the unbroken threshold value, and the current parameter value.

## ThreshMinO, ThreshMaxO, ThreshProgO, and ThreshProgOKO

These work the same as their *I counterparts, except on the Output (second) parameter.

Note that you can use the SetEnv parameter explained above to pass additional information to the threshold programs.

## SetEnv

When calling threshold scripts from within your cfg file you might want to pass some data on to the script. This can be done with the SetEnv configuration option which takes a series of environment variable assignments. Note that the quotes are mandatory. This does not work for external scripts. It is not possible to set environment variables per target.

Example:

     SetEnv[myrouter]:  EMAIL="contact_email@someplace.net"
                        HOST="www.some_server.net"
                        URL="http://www.some_server.net/path/mrtg.html";

# PER TARGET DEFAULT VALUES

## Pre- and Postfix

To save yourself some typing you can define a target called '^'. The text of every Keyword you define for this target will be PREPENDED to the corresponding Keyword of all the targets defined below this line. The same goes for a Target called '$' but its text will be APPENDED.

Note that a space is inserted between the prepended text and the Keyword value, as well as between the Keyword value and the appended text. This works well for text-valued Keywords, but is not very useful for other Keywords. See the ``default'' target description below.

The example will make mrtg use a common header and a common contact person in all the pages generated from targets defined later in this file.

Example:

     PageTop[^]: <H1>NoWhere Unis Traffic Stats</H1><HR>
     PageTop[$]: Contact Peter Norton if you have any questions<HR>

To remove the prepend/append value, specify an empty value, e.g.:

     PageTop[^]:
     PageTop[$]:

## NoSpaceChar

With PREPEND and APPEND (see below) there is normally a space inserted between the local value and the PRE- or APPEND value. Sometimes this is not desirable. You can use the global option NoSpaceChar to define a character which can be mentioned at the end of a $ or ^ definition in order to supress the space.

Example:

      NoSpaceChar: ~
      Target[^]: 1.3.6.1.4.1.482.50.2.4.20.0&1.3.6.1.4.1.482.50.2.4.21.0:get@~
      Target[a]: a.tolna.net
      Target[b]: b.tolna.net
      Target[c]: c.tolna.net
      Target[d]: d.tolna.net

## Default Values

The target name '_' specifies a default value for that Keyword. In the absence of explicit Keyword value, the prepended and the appended keyword value, the default value will be used.

Example:

     YSize[_]: 150
     Options[_]: growright,bits,nopercent
     WithPeak[_]: ymw
     Suppress[_]: y
     MaxBytes[_]: 1250000

To remove the default value and return to the 'factory default', specify an empty value, e.g.:

     YLegend[_]:

There can be several instances of setting the default/prepend/append values in the configuration file. The later setting replaces the previous one for the rest of the configuration file. The default/prepend/append values used for a given keyword/target pair are the ones that were in effect at the point in the configuration file where the target was mentioned for the first time.

Example:

     MaxBytes[_]: 1250000
     Target[myrouter.somplace.edu.2]: 2:public@myrouter.somplace.edu
     MaxBytes[_]: 8000
     Title[myrouter.somplace.edu.2]: Traffic Analysis for myrouter.somplace.edu IF 2

The default MaxBytes for the target myrouter.someplace.edu.2 in the above example will be 1250000, which was in effect where the target name myrouter.someplace.edu.2 first appeared in the config file.

# COMMAND LINE OPTIONS

--user username and --group groupname
  Run as the given user and/or group. (Unix Only)

--lock-file filename
  Use an alternate lock-file (the default is to use the configuration-file appended with `_l`).

--confcache-file filename
  Use an alternate confcache-file (the default is to use the configuration-file appended with `.ok`)

--logging filename|eventlog
  If this is set to writable filename, all output from mrtg (warnings, debug messages, errors) will go to filename. If you are running on Win32 you can specify eventlog instead of a filename which will send all error to the windows event log.

  NOTE:Note, there is no Message DLL for mrtg. This has the side effect that the windows event logger will display a nice message with every entry in the event log, complaing about the fact that mrtg has no message dll. If any of the Windows folks want to contribute one, they are welcome.

--daemon
  Put MRTG into the background, running as a daemon. This works the same way as the config file option, but the switch is required for proper FHS operation (because /var/run is writable only by root)

--fhs
  Configure all mrtg paths to conform to the FHS specification; http://www.pathname.com/fhs/

--check
  Only check the cfg file for errors. Do not do anything.

--pid-file=s
  Define the name and path of the pid file for mrtg running as a daemon

--debug=s
  Enable debug options. The argument of the debug option is a comma separated list of debug values:

       cfg  - watch the config file reading
       dir  - directory mangeling
       base - basic program flow
       tarp - target parser
       snpo - snmp polling
       fork - forking view
       time - some timing info
       log  - logging of data via rateup or rrdtool

  Example:

       --debug="cfg,snpo"

# EXAMPLES

## Minimal mrtg.cfg

     WorkDir: /usr/tardis/pub/www/stats/mrtg
     Target[r1]: 2:public@myrouter.somplace.edu
     MaxBytes[r1]: 8000
     Title[r1]: Traffic Analysis ISDN
     PageTop[r1]: <H1>Stats for our ISDN Line</H1>

## Cfg for several Routers.

     WorkDir: /usr/tardis/pub/www/stats/mrtg
     Title[^]: Traffic Analysis for
     PageTop[^]: <H1>Stats for
     PageTop[$]: Contact The Chief if you notice anybody<HR>
     MaxBytes[_]: 8000
     Options[_]: growright

     Title[isdn]: our ISDN Line
     PageTop[isdn]: our ISDN Line</H1>
     Target[isdn]: 2:public@router.somplace.edu

     Title[backb]: our Campus Backbone
     PageTop[backb]: our Campus Backbone</H1>
     Target[backb]: 1:public@router.somplace.edu
     MaxBytes[backb]: 1250000

     # the following line removes the default prepend value
     # defined above

     Title[^]:

     Title[isdn2]: Traffic for the Backup ISDN Line
     PageTop[isdn2]: our ISDN Line</H1>
     Target[isdn2]: 3:public@router.somplace.edu

# AUTHOR

Tobias Oetiker <oetiker@ee.ethz.ch> and many contributors