MRTG-NT-GUIDE(1)               mrtg              MRTG-NT-GUIDE(1)



NNAAMMEE
       mrtg-nt-guide - The Windows Guide to MRTG 2.14.4

SSYYNNOOPPSSIISS
       Installing MRTG on a Windows box is not quite as "click
       and point" as some might want it to be. But then again, it
       is not all that difficult if you follow the instructions
       below.

PPRREERREEQQUUIISSIITTEESS
       To get MRTG to work on Windows you need the following:

       +o   A current copy of Perl.  For Example ActivePerl from
           http://www.activestate.com/Products/Download/Down-
           load.plex?id=ActivePerl

       +o   The latest version of MRTG from
           http://oss.oetiker.ch/mrtg/pub Look for
           mrtg-2.14.4.zip or better. The archive also contains a
           precompiled copy of rateup.exe for Win32.

IINNSSTTAALLLLIINNGG
       I suggest you do the following from the machine that will
       be running MRTG, which, in this case, is also a web
       server. All examples are for doing things to a LOCAL
       machine.

       First
           Unzip MRTG to C:\mrtg-2.14.4 on the Windows machine of
           your choice.

       Next
           Install Perl on the same Windows machine. You might
           want to make sure that the Perl binary directory is
           listed in your system path.

            C:\Perl\bin;%SystemRoot%\system32;%SystemRoot%;...

           You can manually check this by going to [Control
           Panel]->[System]->[Environment]

       To see if everything is installed properly you can open a
       Command Shell and go into _c_:_\_m_r_t_g_-_2_._1_4_._4_\_b_i_n. Type:

        perl mrtg

       This should give you a friendly error message complaining
       about the missing MRTG configuration file. Now, you have
       successfully installed MRTG and Perl.

CCOONNFFIIGGUURRIINNGG MMRRTTGG
       Now it is time to create a configuration for MRTG. But
       before we begin you need to know a few things. Take an
       opportunity to gather the following information:

       +o   The IP address or hostname and the SNMP port number,
           (if non standard), of the device you want to monitor.

       +o   If you want to monitor something other than bytes in
           and out, you must also know the SNMPOID of what you
           want to monitor.

       +o   Finally you need to know the read-only SNMP community
           string for your device. If you don't know it, try ppuubb--
           lliicc, that is the default.

       For the rest of this document we will be using device
       1100..1100..1100..11 ( a CISCO Catalyst 5000) with Community string
       ppuubblliicc. We are interested in monitoring traffic, and the
       CPU load. Let's begin.

       The first thing we do in setting up MRTG is making a
       default config file.  Get to a cmd prompt and change to
       the _c_:_\_m_r_t_g_-_2_._1_4_._4_\_b_i_n directory. Type the following com-
       mand:

        perl cfgmaker public@10.10.10.1 --global "WorkDir: c:\www\mrtg" --output mrtg.cfg

       This creates an initial MRTG config file for you. Note
       that in this file all interfaces of your router will be
       stored by number. Unfortunately, these numbers are likely
       to change whenever you reconfigure your router. In order
       to work around this you can get _c_f_g_m_a_k_e_r to produce a con-
       figuration which is based on Ip numbers, or even Interface
       Descriptions. Check cfgmaker

       If you get an error message complaining about nnoo ssuucchh nnaammee
       or nnoo rreessppoonnssee, your community name is probably wrong.

       Now, let's take a look at the mrtg.cfg file that was cre-
       ated.

       In Perl, a "#" is a comment, synonymous with "REM" in DOS.

       Add the following to the top of the mrtg.cfg file:

        WorkDir: D:\InetPub\wwwroot\MRTG

       This is where the web pages are created, usually a web
       root.

        ######################################################################
        # Description: LCP SUWGB
        # Contact: Administrator
        # System Name: LC-Bridge
        # Location: Here
        #.....................................................................

       TargetDevice's IP Address:Interface Number:Community:IP
       Address

        Target[10.10.10.1.1]: 1:public@10.10.10.1

       This is the interface speed (Default is 10 megabits; for
       100Mbit devices use 12500000 and so on...)

        MaxBytes[10.10.10.1.1]: 1250000

        Title[10.10.10.1.1]: LC-Bridge (sample.device): ether0

       This section determines how the web page headers will look







        PageTop[10.10.10.1.1]: <H1>Traffic Analysis for ether0</H1>
         <TABLE>
         <TR><TD>System:</TD><TD>LC-Bridge inAndover</TD></TR>
         <TR><TD>Maintainer:</TD><TD>Administrator</TD></TR>
         <TR><TD>Interface:</TD><TD>ether0(1)</TD></TR>
         <TR><TD>IP:</TD><TD>sample.device(10.10.10.1)</TD></TR>
         <TR><TD>Max Speed:</TD>
         <TD>1250.0 kBytes/s (ethernetCsmacd)</TD></TR>
         </TABLE>

         Target[10.10.10.1.2]: 2:public@10.10.10.1
         MaxBytes[10.10.10.1.2]: 1250000
         Title[10.10.10.1.2]: LC-Bridge (): ulink0
         PageTop[10.10.10.1.2]: <H1>Traffic Analysis for ulink0</H1>
          <TABLE>
          <TR><TD>System:</TD><TD>LC-Bridge inAndover</TD></TR>
          <TR><TD>Maintainer:</TD><TD>Administrator</TD></TR>
          <TR><TD>Interface:</TD><TD>ulink0(2)</TD></TR>
          <TR><TD>IP:</TD><TD>()</TD></TR>
          <TR><TD>Max Speed:</TD>
          <TD>1250.0 kBytes/s (ethernetCsmacd)</TD></TR>
          </TABLE>

         #---------------------------------------------------------------

       And that's a very basic MRTG config file. You can run this
       and see your results by going into the _c_:_\_m_r_t_g_-_2_._1_4_._4_\_b_i_n
       directory and typing:

        perl mrtg mrtg.cfg

       It is normal to get errors for the first two times you run
       this command. The errors will alert you about the fact
       that there have not been any log files in existence
       before.

       If you take a look at those web pages they are not very
       exciting (yet). You need to have the MRTG files run every
       five minutes to produce the desired results.  Just run it
       again after a few minutes. You should now be able to see
       the first lines in your graphs.

MMAAKKEE MMRRTTGG RRUUNN AALLLL TTHHEE TTIIMMEE
       Starting MRTG by hand every time you want to run it is not
       going to make you happy I guess.

       There is a special option you can set in the MRTG configu-
       ration file so so that MRTG will not terminate after it
       was started. Instead it will wait for 5 minutes and then
       run again.

       Add the option

        RunAsDaemon: yes

       to your mrtg.cfg file and start it with:

        start /Dc:\mrtg-2.14.4\bin wperl mrtg --logging=eventlog mrtg.cfg

       If you use wwppeerrll instead of ppeerrll, no console window will
       show. MRTG is now running in the background. If it runs
       into problems it will tell you so over the EventLog. To
       stop MRTG, open the Task Manager and terminate the
       wwppeerrll..eexxee process. If mrtg has anything to tell you these
       messages can be found in the event log.

       If you put a shortcut with

        Target:    wperl mrtg --logging=eventlog mrtg.cfg
        Start in:  c:\mrtg-2.14.4\bin

       into your start-up folder, MRTG will now start whenever
       you login to your NT box.

       If you do not want to log into your box just to start
       MRTG. Have a look at http://www.firedae-
       mon.com/mrtg-howto.html which describes a free tool to
       start any program as a Service. The pages gives specific
       instructions for MRTG users.

HHOOWW TTOO SSEETTUUPP MMRRTTGG AASS AA WWIINNDDOOWWSS SSEERRVVIICCEE
       AAddddiittiioonnaall PPrreerreeqquuiissiitteess


       +o   MRTG must be installed and fully configured on the
           target system.  In the following exercise the assump-
           tion is that MRTG is installed under c:\mrtg\ and all
           the sample files use this location.

       +o   Microsoft Tools SSRRVVAANNYY..eexxee (Applications as Services
           Utility) and IINNSSTTSSRRVV..eexxee (Service Installer) - Those
           files can be downloaded from Microsoft as a part of
           Windows 2000 Resource Kit at
           <http://www.microsoft.com/windows2000/tech-
           info/reskit/tools/default.asp>.  They are also avail-
           able from other locations such as <http://www.electra-
           soft.com/srvany/srvany.htm>,
           <http://www.iopus.com/guides/srvany.htm>, etc.
           Detailed instructions on how to use this package are
           available at <http://sup-
           port.microsoft.com/kb/q137890/>.  In order to follow
           the steps in this HOW-TO you MMUUSSTT obtain both executa-
           bles.

       +o   You must have administrative rights on the target sys-
           tem.

       PPrreeppaarraattiioonn

       Please complete the following steps before starting the
       installation:

       +o   Copy ssrrvvaannyy..eexxee and iinnssttssrrvv..eexxee to c:\mrtg\bin\ (your
           MRTG bin directory).

       +o   Create a file called mmrrttgg..rreegg anywhere on your system
           and paste the following content into it:

            Windows Registry Editor Version 5.00

            [HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\MRTG\Parameters]
            "Application"="c:\\perl\\bin\\wperl.exe"
            "AppParameters"="c:\\mrtg\\bin\\mrtg --logging=eventlog c:\\mrtg\\bin\\mrtg.cfg"
            "AppDirectory"="c:\\mrtg\\bin\\"

       SSeerrvviiccee IInnssttaallllaattiioonn

       Once again, assuming that MRTG is already fully installed
       and configured on the target system under c:\mrtg\ the
       following steps are necessary to setup MRTG as a service.

       Using the command prompt go into the temporary directory
       where you unzipped the package.  When there type the fol-
       lowing command to create a service named "MRTG" in the
       Windows Services management console:

        instsrv MRTG c:\mrtg\bin\srvany.exe

       Now you need to create the AApppp** entries required for the
       new service.  You can do this by either right-clicking on
       the mrtg.reg file and selecting 'merge' or by running the
       following command:

        regedit /s mrtg.reg

       After setting up the registry entry it is time to point it
       to your MRTG installation.  If you have installed MRTG
       under _c_:_\_m_r_t_g_\, you can skip this step.  Open your reg-
       istry editor (Start -> Run -> regedt32), and locate the
       [[HHKKEEYY__LLOOCCAALL__MMAACCHHIINNEE\\SSYYSSTTEEMM\\CCuurrrreennttCCoonnttrroollSSeett\\SSeerr--
       vviicceess\\MMRRTTGG]] key.  Make sure that the IImmaaggeePPaatthh variable is
       correctly pointing to ssrrvvaannyy..eexxee located in your MRTG bin
       directory (for example c:\mrtg\bin\srvany.exe).  Next you
       have to expand the MRTG tree, and go to the
       [[HHKKEEYY__LLOOCCAALL__MMAACCHHIINNEE\\SSYYSSTTEEMM\\CCuurrrreennttCCoonnttrroollSSeett\\SSeerr--
       vviicceess\\MMRRTTGG\\PPaarraammeetteerrss]] key.  Under Parameters make sure
       that all the  AApppplliiccaattiioonn variables are setup properly.

       At this point you are ready to run the service.  The only
       thing left to do is to start the MRTG service in the Ser-
       vices management console.  After you do this, you should
       see two new processes running on your system: srvany.exe
       and wperl.exe.  Make sure to stop any previously running
       MRTG processes to avoid conflict.

       Note that it is imperative to set the RRuunnAAssDDaaeemmoonn:: yyeess
       option or the service will stop after just one single run!

EEXXAAMMPPLLEE
       Now lets look at a config file to monitor what we wanted
       to on our mythical Cisco Cat 5000 -- utilization on ports
       3, 5, 10, and 24, and the CPU Load, which will show us
       nonstandard mrtg configurations as well as more options..

        WorkDir: D:\InetPub\wwwroot\MRTG
        RunAsDaemon: yes

        ######################################################################
        # Description: LCP SUWGB
        # Contact: Administrator
        # System Name: LC-Bridge
        # Location: Here
        #.....................................................................

        Target[10.10.10.1.1]: 3:public@10.10.10.1
        MaxBytes[10.10.10.1.1]: 1250000
        Title[10.10.10.1.1]: LC-Bridge (sample-device): ether0
        PageTop[10.10.10.1.1]: <H1>Traffic Analysis for ether0</H1>
         <TABLE>
        <TR><TD>System:</TD><TD>LC-Bridge inAndover</TD></TR>
        <TR><TD>Maintainer:</TD><TD>Administrator</TD></TR>
        <TR><TD>Interface:</TD><TD>ether0(3)</TD></TR>
        <TR><TD>IP:</TD><TD>sample-device(10.10.10.1)</TD></TR>
        <TR><TD>Max Speed:</TD>
        <TD>1250.0 kBytes/s (ethernetCsmacd)</TD></TR>
        </TABLE>

        #---------------------------------------------------------------

        Target[10.10.10.1.2]: 5:public@10.10.10.1
        MaxBytes[10.10.10.1.2]: 1250000
        Title[10.10.10.1.2]: LC-Bridge (): ulink0
        PageTop[10.10.10.1.2]: <H1>Traffic Analysis for ulink0</H1>
         <TABLE>
         <TR><TD>System:</TD><TD>LC-Bridge inAndover</TD></TR>
         <TR><TD>Maintainer:</TD><TD>Administrator</TD></TR>
         <TR><TD>Interface:</TD><TD>ulink0(5)</TD></TR>
         <TR><TD>IP:</TD><TD>()</TD></TR>
         <TR><TD>Max Speed:</TD>
         <TD>1250.0 kBytes/s (ethernetCsmacd)</TD></TR>
         </TABLE>

        #---------------------------------------------------------------

        Target[10.10.10.1.1]: 10:public@10.10.10.1
        MaxBytes[10.10.10.1.1]: 1250000
        Title[10.10.10.1.1]: LC-Bridge (sample-device): ether0
        PageTop[10.10.10.1.1]: <H1>Traffic Analysis for ether0</H1>
         <TABLE>
         <TR><TD>System:</TD><TD>LC-Bridge inAndover</TD></TR>
         <TR><TD>Maintainer:</TD><TD>Administrator</TD></TR>
         <TR><TD>Interface:</TD><TD>ether0(10)</TD></TR>
         <TR><TD>IP:</TD><TD>sample-device(10.10.10.1)</TD></TR>
         <TR><TD>Max Speed:</TD>
         <TD>1250.0 kBytes/s (ethernetCsmacd)</TD></TR>
         </TABLE>

        #---------------------------------------------------------------

        Target[10.10.10.1.2]: 24:public@10.10.10.1
        MaxBytes[10.10.10.1.2]: 1250000
        Title[10.10.10.1.2]: LC-Bridge (): ulink0
        PageTop[10.10.10.1.2]: <H1>Traffic Analysis for ulink0</H1>
         <TABLE>
         <TR><TD>System:</TD><TD>LC-Bridge inAndover</TD></TR>
         <TR><TD>Maintainer:</TD><TD>Administrator</TD></TR>
         <TR><TD>Interface:</TD><TD>ulink0(24)</TD></TR>
         <TR><TD>IP:</TD><TD>()</TD></TR>
         <TR><TD>Max Speed:</TD>
         <TD>1250.0 kBytes/s (ethernetCsmacd)</TD></TR>
         </TABLE>

        #---------------------------------------------------------------

        # Router CPU load %
        Target[cpu.1]:1.3.6.1.4.1.9.2.1.58.0&1.3.6.1.4.1.9.2.1.58.0:public@10.10.10.1
        RouterUptime[cpu.1]: public@10.10.10.1
        MaxBytes[cpu.1]: 100
        Title[cpu.1]: CPU LOAD
        PageTop[cpu.1]: <H1>CPU Load %</H1>
        Unscaled[cpu.1]: ymwd
        ShortLegend[cpu.1]: %
        XSize[cpu.1]: 380
        YSize[cpu.1]: 100
        YLegend[cpu.1]: CPU Utilization
        Legend1[cpu.1]: CPU Utilization in % (Load)
        Legend2[cpu.1]: CPU Utilization in % (Load)
        Legend3[cpu.1]:
        Legend4[cpu.1]:
        LegendI[cpu.1]:
        LegendO[cpu.1]: &nbsp;Usage
        Options[cpu.1]: gauge

       This is a nice example of how to monitor any SNMP device
       if you know what OID you want to use. Once again, for an
       explanation of the more advance features of mrtg, please
       see the rest of the documentation.

AAUUTTHHOORRSS
       Tobi Oetiker <tobi@oetiker.ch>, David S. Divins <ddi-
       vins@moon.jic.com>, Steve Pierce <MRTG@HDL.com>, Artyom
       Adjemov <one.bofh@gmail.com>, Ilja Ivanov <ivanov@bseu.by>
       Karel Fajkus <karel@fajkus.cz>



2.14.4                      2006-07-04           MRTG-NT-GUIDE(1)
