# Monitoring Cisco BPX ATM Switches with MRTG:

<[!if !supportEmptyParas]> <[!endif]>

### These OIDs work for monitoring total cells transmitted and received on a trunk on the Cisco BPX Switch.

X=slot number Y=1st digit of port number Z=2nd digit of port number(If single digit number ie.8, Z=0)

<[!if !supportEmptyParas]> <[!endif]>

.1.3.6.1.4.1.351.100.4.2.4.4.1.25.X0YZ000

atmTrkStatsTotalCellsTxtoLns

<[!if !supportEmptyParas]> <[!endif]>

OBJECT-TYPE -- FROM STRATACOM-MIB

SYNTAX Counter

MAX-ACCESS read-only

STATUS Mandatory

DESCRIPTION "The number of total cells transmitted to the line."

::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) stratacom(351) snmpAgents(100) strmSwitchMIB(4) switchServiceObjects(2) trunkServiceObjects(4) atmTrunkStatsTable(4) atmTrkStatsEntry(1) atmTrkStatsTotalCellsTxtoLns(25)

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

.1.3.6.1.4.1.351.100.4.2.4.4.1.26.X0YZ000

atmTrkStatsTotalCellsRxFromPorts

<[!if !supportEmptyParas]> <[!endif]>

OBJECT-TYPE-- FROM STRATACOM-MIB

SYNTAX Counter

MAX-ACCESS read-only

STATUS Mandatory

DESCRIPTION "The number of total cells received from the port."

::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) stratacom(351) snmpAgents(100) strmSwitchMIB(4) switchServiceObjects(2) trunkServiceObjects(4) atmTrunkStatsTable(4) atmTrkStatsEntry(1) atmTrkStatsTotalCellsRxFromPorts(26)

<[!if !supportEmptyParas]> <[!endif]>

example MRTG.cfg entry:

Target[Switchname_2.1]:.1.3.6.1.4.1.351.100.4.2.4.4.1.25.X0YZ000&.1.3.6.1.4.1.351.100.4.2.4.4.1.26.X0YZ000:community@x.x.x.x*53

#multiply above by 53(53 bytes in a cell)

Options[Switchname_2.1]:bits

PageTop[ Switchname_2.1]:<H1>Traffic for switchname, FDR trunk 2.1 to switchname(MGX)</H1>

AbsMax[Switchname_2.1]:149759768

MaxBytes[Switchname_2.1]:149759768

Directory[Switchname_2.1]:xxxxx

Ylegend[Switchname_2.1]:Bits per second

ShortLegend[Switchname_2.1]:bps

Title[Switchname_2.1]:Traffic for Switchname, FDR trunk 2.1 to switchname(MGX)

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

### These OIDs work for monitoring total cells transmitted and received on a port on the Cisco BPX Switch.

X=slot number Y=port number

<[!if !supportEmptyParas]> <[!endif]>

.1.3.6.1.4.1.351.100.4.2.2.3.1.8.X.Y

atmPortStatCellsRxs OBJECT-TYPE

-- FROM STRATACOM-MIB

SYNTAX Counter

MAX-ACCESS read-only

STATUS Mandatory

DESCRIPTION "Total numbers of cells received."

::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) stratacom(351) snmpAgents(100) strmSwitchMIB(4) switchServiceObjects(2) atmServiceObjects(2) atmPortStatTable(3) atmPortStatEntry(1) 8 }

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

.1.3.6.1.4.1.351.100.4.2.2.3.1.12.X.Y

atmPortStatCellsTxs OBJECT-TYPE

-- FROM STRATACOM-MIB

SYNTAX Counter

MAX-ACCESS read-only

STATUS Mandatory

DESCRIPTION "Total numbers of cells transmitted."

::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) stratacom(351) snmpAgents(100) strmSwitchMIB(4) switchServiceObjects(2) atmServiceObjects(2) atmPortStatTable(3) atmPortStatEntry(1) 12 }

<[!if !supportEmptyParas]> <[!endif]>

Example MRTG.cfg entry:

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

Target[SYRTGB01_6.10]:.1.3.6.1.4.1.351.100.4.2.2.3.1.8.6.10&.1.3.6.1.4.1.351.100.4.2.2.3.1.12.6.10:public@10.1.1.34*53

#multiply cells by 53 to convert to bytes

Options[Switchname_6.10]:bits

PageTop[Switchname_6.10]:<H1>Port Bandwidth DS-3</H1>

MaxBytes[Switchname_6.10]:4608000

Directory[Switchname_6.10]:xxxxxx

Ylegend[Switchname_6.10]:Bits per second

ShortLegend[Switchname_6.10]:bps

Title[Switchname_6.10]:Port Bandwidth DS-3

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

# Monitoring Cisco MGX Frame Relay connections with MRTG:

### These OIDs work for monitoring total cells transmitted and received on a port on the Cisco BPX Switch.

<[!if !supportEmptyParas]> <[!endif]>

.1.3.6.1.4.1.351.110.2.5.1.1.4.1

xmtCells OBJECT-TYPE

-- FROM AXIPOP-MIB

SYNTAX Counter

MAX-ACCESS read-only

STATUS Mandatory

DESCRIPTION "The number of cells transmitted on this channel."

::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) stratacom(351) basis(110) cardGeneric(2) sarChannelCounter(5) sarChannelCounterTable(1) sarChannelCounterEntry(1) xmtCells(4) 1 }

<[!if !supportEmptyParas]> <[!endif]>

.1.3.6.1.4.1.351.110.2.5.1.1.12.1

rcvCells OBJECT-TYPE

-- FROM AXIPOP-MIB

SYNTAX Counter

MAX-ACCESS read-only

STATUS Mandatory

DESCRIPTION "The number of cells that were received on this channel."

::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) stratacom(351) basis(110) cardGeneric(2) sarChannelCounter(5) sarChannelCounterTable(1) sarChannelCounterEntry(1) rcvCells(12) 1 }

<[!if !supportEmptyParas]> <[!endif]>

<[!if !supportEmptyParas]> <[!endif]>

######enterprises.351.110.2.5.1.1.4.1.x.yy =Transmit Cells from SAR

######enterprises.351.110.2.5.1.1.12.1.x.yy =Recieve Cells from SAR

######x=slotnumber

######yy=channel number

<[!if !supportEmptyParas]> <[!endif]>

Target[Switchname_11_142]:enterprises.351.110.2.5.1.1.4.1.x.yy&enterprises.351.110.2.5.1.1.12.1.x.yy:POPEYE\@SM_11@10.1.1.35*53

#\@ the \breaks out of Perl so the @ is not processedthanks Tobi.

#POPEYE is always the community name of the switch, SM_11 means service module 11, if you need stats from #the active PXM the community is POPEYE@PXM_ACTIVE

Options[Switchname_11_142]: bits

PageTop[Switchname_11_142]:<H1>xxxx Frame Statistics</H1>

AbsMax[Switchname_11_142]:1536000

#Port Speed

MaxBytes[Switchname_11_142]:1536000

#MaxBytes=CIR

Directory[Switchname_11_142]:xxxx

Ylegend[Switchname_11_142]:Bits per second

ShortLegend[Switchname_11_142]:bps

Title[Switchname_11_142]: 11.19.0.17 DLCI 17