From webmaster@hiway.com.br Fri Feb 16 23:24:20 2001
From: Fernando Braghetto - Webmaster Hiway <webmaster@hiway.com.br>
To: oetiker@ee.ethz.ch
Date: Thu, 15 Feb 2001 09:51:27 -0300
Subject: [Contribution] TCH Modem


    [ Part 1.1, Text/PLAIN  86 lines. ]
    [ Unable to print this part. ]

Tobias,
 
    I want to contrib with the MRTG.
    I do not have time for add this to indexmaker / cfgmaker. Sorry!
   
    Actually I'm found some very good Objects IDs for the Total Control
Modem Racks (3Com).
 
    To make management for the number of users connected in a HyperARC
card (with HyperDSP modem) or Netserver card (with Quad-Modens and
DualPri card) use this cfg:
    (sorry for my bad english)
 

# Example of configuration by
# Fernando Braghetto/Brazil - braghetto@hiway.com.br
# created in Feb/15 2001
 
# TotalControl Temperature
# change the IP Address 10.0.0.1 with the IP of Hyper NMC card (Network
Management Card)
#
Target[TCTemp]:
1.3.6.1.4.1.429.1.2.2.5.0&1.3.6.1.4.1.429.1.2.2.5.0:public@10.0.0.1
MaxBytes[TCTemp]: 36
Title[TCTemp]: Temperature
ShortLegend[TCTemp]: ēC
Unscaled[TCTemp]: ymwd
YLegend[TCTemp]: Temperature
LegendI[TCTemp]: &nbsp;System Temp&nbsp;
LegendO[TCTemp]: &nbsp;System Temp&nbsp;
Options[TCTemp]: gauge
PageTop[TCTemp]:
      <font face="Verdana">
      <H2>Temperatura do TotalControl E1</H2>
 
 
 
# TotalControl Connected Users in HyperARC (using HyperDSP E1 modens)
# change the IP Address 10.0.0.2 with the IP of Hyper ARC card (Routing
Card)
#
Target[TCHDSP]:
1.3.6.1.4.1.429.4.2.1.10.0&1.3.6.1.4.1.429.4.2.1.10.0:public@10.0.0.2:
MaxBytes[TCHDSP]: 420
Title[TCHDSP]: Connected Users
ShortLegend[TCHDSP]: Users
YLegend[TCHDSP]: Users
LegendI[TCHDSP]: &nbsp;Connected Users&nbsp;
LegendO[TCHDSP]: &nbsp;Connected Users&nbsp;
Options[TCHDSP]: gauge
PageTop[TCHDSP]:
      <font face="Verdana">
 <H2>Number of Connected Users</H2>
 
 
 
# TotalControl Connected Users in Netserver Card (using Quad modens and
Dual Pri Card)
# change the IP Address 10.0.0.3 with the IP of Netserver card (Routing
Card)
#
Target[TCNetserver]: 1.3.6.1.2.1.2.1.0&1.3.6.1.2.1.2.1.0:public@10.0.0.3
MaxBytes[TCNetserver]: 56
Title[TCNetserver]: Connected Users
ShortLegend[TCNetserver]: Users
Unscaled[TCNetserver]: ymwd
YLegend[TCNetserver]: Users
Legend1[TCNetserver]: Users
Legend2[TCNetserver]: Users
Legend3[TCNetserver]: Users
Legend4[TCNetserver]: Users
LegendI[TCNetserver]: &nbsp;Digital Connections&nbsp;
LegendO[TCNetserver]: &nbsp;Analog Connections&nbsp;
Options[TCNetserver]: gauge
PageTop[TCNetserver]:
      <font face="Verdana">
 <H2>Number of Connected Users</H2>
 
 
Sincerly,
Fernando Braghetto
IT Manager, Network Admin, Webmaster
Hiway Internet Provider - Brazil
[IMAGE] 


    [ Part 2, Image/GIF  7.6KB. ]
    [ Unable to print this part. ]

